SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CRH5A_6
	Type ( Engine )
	WagonShape ( CRH5A_6.s )
	size ( 3.0m 3.40m 26m)  
	Mass ( 58t )
	WheelRadius ( 0.4575m )
	InertiaTensor ( Box ( 3.0m 3.40m 26m) )
        Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 9e6N/m 5e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 3cm 5cm )
		)
		CouplingHasRigidConnection ()
		CouplingUniqueType ( "CRH5_5M+3T" )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 9e6N/m 5e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 3cm 5cm )
		)
		CouplingHasRigidConnection ()
	)
	Buffers (
		Spring (
			Stiffness ( 1e7N/m 0 )
			Damping ( 2e6N/m/s 0 )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.0 )
		Radius ( 1 )
		Angle ( 0.4deg )
	)

	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 309.32kN )
	DerailBufferForce ( 535.82kN )
	NumWheels ( 1 )
	Friction (
		100N/m/s		0		1mph		9.16N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		        1
	)

	BrakeEquipmentType( "EP_brake" )
	BrakeSystemType( "EP" )
	MaxBrakeForce( 25.7KN )

	EmergencyBrakeResMaxPressure( 65.3 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 7.25 )
	MaxApplicationRate( 8.47 )
	MaxAuxilaryChargingRate( 7.25 )
	EmergencyResCapacity( 10 )
	EmergencyResChargingRate( 29 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 43.54 )
	
	Sound ( "GenPassWagModern.sms" )

)

Engine ( CRH5A_6
	Wagon ( CRH5A_6 )
	Type ( Electric )
	MaxPower ( 1100kW )
	MaxForce ( 150kN )
	MaxContinuousForce ( 130kN )
	MaxVelocity ( 200kmh )
	MaxCurrent ( 2500A )
	WheelRadius ( 0.5m )
	Sanding ( 2kmh )
	NumWheels ( 1 )

	AirBrakesAirCompressorPowerRating( 3 )
	AirBrakesMainMinResAirPressure( 108.78 )
	AirBrakesMainMaxAirPressure( 130.53 )
	AirBrakesMainResVolume( 42.8 )
	AirBrakesAirCompressorWattage( 22000 )
	AirBrakesCompressorRestartPressure( 108.78 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.22 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	TrainBrakesControllerMaxApplicationRate( 7.257 )
	TrainBrakesControllerMaxReleaseRate( 4.1 )
	TrainBrakesControllerEmergencyApplicationRate( 34.83 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 87.02 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerFullServicePressureDrop( 24.65 )

	DynamicBrakesMinUsableSpeed( 0 )
	DynamicBrakesMaximumEffectiveSpeed( 23 )
	DynamicBrakesMaximumForce( 130kN )
	DynamicBrakesResistorCurrentLimit ( 920 )
	DynamicBrakesCutInSpeed( 0 )
	DynamicBrakesMaxAirBrakePressure ( 15 )
	DynamicBrakesFadingSpeed( 46 )
	DynamicBrakesDelayTimeBeforeEngaging ( 1 )
	DynamicBrakesMaximumSpeedForFadeOut ( 99.36 )
	DynamicBrakesEffectAtMaximumFadeOut( 0.2 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 10 )
	DynamicBrakeHasAutoBailOff( 1 )


	BrakesEngineControllers( "Train" )
        BrakesEngineControllers( "Independent, Train, Dynamic" )

	DoesBrakeCutPower( 1 )
	DoesHornTriggerBell( 0 )
	BrakeCutsPowerAtBrakeCylinderPressure( 14.5 )
        DieselEngineSpeedOfMaxTractiveEffort( 150 )

    	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)
		
	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 40 )
		MonitoringDeviceAlarmTimeLimit( 30 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 139 )
		MonitoringDeviceResetLevel( -1 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		)
	
        EngineControllers (
           Throttle ( 0 1 0.1 0 
                NumNotches ( 1 
                    Notch ( 0        1 Dummy )
                    )
            )
            Brake_Train ( 0 1 0.05 0
                NumNotches ( 5
                    Notch ( 0    0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.25 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.85 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
                )
            )

            Brake_Dynamic ( 0 1 0.1 0 
                NumNotches ( 1
                    Notch ( 0       1 Dummy )
                )
            )

	    Combined_Control( 0 1 0.5 0.5 throttle dynamic )
            DirControl ( -1 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )

    	Sound ( "CRH5CAB.sms" )
    	Name ( "CRH5A_6" )
        Description (
	
       "airy1982@163.com\n"     )  
        EngineOperatingProcedures (
        "To move forward\n"+
        "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
	"2.	Press the W key to move the Reverser to Forward.\n"+
	"3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"4. 	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"5.	Press the D key to move increase the Throttle setting.\n\n"+  
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
		"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key and the [ (LEFT BRACKET) key to release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the 'permission to depart' signal.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
        ) 
)
