SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 50ft_flat_wsor  
	comment( 50ft_flat_wsor )
	Type ( Freight )
	WagonShape ( 50ft_flat_wsor.s )
	Size ( 3.1m 1.5m 16.5m)
	comment( 27.21t empty, 97.1t full metric )
	Mass ( "27.21t" )
	WheelRadius ( 36in/2 )
	InertiaTensor ( Box (3m 1.5m 16.5m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m 1e6N/m )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 20cm 30cm )
		)
		comment( CouplingHasRigidConnection () )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*74t )
	DerailBufferForce ( 400kN )
	NumWheels (	8 )
	Friction (
		100N/m/s		1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)

	Lights	(	1
		Light	(
			comment( Rear red light flashing - night )
			Type		( 0 )
			Conditions	(
				Unit ( 3 )
				Service ( 2 )
				TimeOfDay ( 2 )
				Coupling ( 1 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	2
				State	(
					Duration ( 0.41 )
					LightColour ( 80ff0000 )
					Position ( 0 1.248 -8.2 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
				State	(
					Duration ( 0.41 )
					LightColour ( 00000000 )
					Position ( 0 1.248 -8.2 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
	)

	BrakeEquipmentType( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 50kN )

	MaxHandbrakeForce( 35kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 25 )
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 7 )
	EmergencyResChargingRate( 5 )
	EmergencyBrakeResMaxPressure( 90 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )
	
  	Sound (	"GenFreightWag3.sms" )
)
