SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( SS9G0094k541
	Type ( Engine )
	WagonShape ( SS9G0094.s )
	Thumbnail ( acthumb1.ace )
 	Size  ( 3.1m 4.6m 21.8m)
	CentreOfGravity ( 0m 2.0m 0m )
	Mass ( 126t )
	WheelRadius ( 0.55m )
	InertiaTensor ( Box (3.1m 4.6m 21.8m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m 1e6N/m )
			Break ( 1.1e7N 1.1e7N )
			r0 ( 15cm 1e9 )
		)
		CouplingHasRigidConnection ()
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)


	comment( guessed brake force )
	MaxBrakeForce ( 150kN )
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 230kN )
	DerailBufferForce ( 200kN )
	NumWheels ( 8 )
	Friction (
		150N/m/s		1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)
	AntiSlip ()
	
	BrakeEquipmentType( "Air_twin_pipe, Distributor" )

	BrakeSystemType( "Air_twin_pipe" )
	

	EmergencyBrakeResMaxPressure( 110 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 20 )
	MaxApplicationRate( 20 )
	MaxAuxilaryChargingRate( 30 )
	EmergencyResCapacity( 10 )
	EmergencyResChargingRate( 30 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	BrakeDistributorFullServicePressure( 82 )
	BrakeDistributorMaxAuxilaryResPressure( 110 )
	BrakeDistributorEmergencyResPressure( 110 )
	BrakeDistributorReleaseRate( 10 )
	BrakeDistributorApplicationRate( 15 )
	BrakeDistributorTrainPipeControlRatio( 2.03 )
	BrakeDistributorNormalFullReleasePressure( 110 )
	Lights	(	20
		Light	(
			comment( Sphere of light )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffff )
					Position ( 0.0 3.5 16.0 )
					Transition ( 0 )
					Radius ( 300.0 )
					Angle ( 10.0 )
					)
				)
			)
		Light	(
			comment( Head light top dim  left)
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c3fb )
					Position ( 0.0 3.75 9.98)
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1 )
					)
				)
			)
		Light	(
			comment( Head light top bright left)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c3fb)
					Position ( 0.0 3.75 9.98)
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1 )
					)
				)
			)
		Light	(
			comment( Head light right bright outer)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b )
					Position ( -1.03 1.92 10.72)
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1 )
					)
				)
			)
		Light	(
			comment( Head light left bright outer)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b )
					Position ( 1.03 1.92 10.72)
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1 )
					)
				)
			)
		Light	(
			comment( Rear red left)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )					Position ( -0.7 1.88 10.61)
					Position ( -0.84 1.92 -10.72)
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Rear red right)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( 0.84 1.92 -10.72)
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light left 10)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( -1.45 1.1 8.0)
					Azimuth ( -90 -90 -90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light left 20)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( -1.45 1.1 3.7)
					Azimuth ( -90 -90 -90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light left 30)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( -1.45 1.1 -3.7)
					Azimuth ( -90 -90 -90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light left 40)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( -1.45 1.1 -8.0)
					Azimuth ( -90 -90 -90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)

		Light	(
			comment( Side light right 10)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( 1.45 1.1 8.0)
					Azimuth ( 90 90 90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light right 20)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( 1.45 1.1 3.7)
					Azimuth ( 90 90 90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light right 30)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( 1.45 1.1 -3.7)
					Azimuth ( 90 90 90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Side light right 40)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c300 )
					Position ( 1.45 1.1 -8.0)
					Azimuth ( 90 90 90 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)

		)
    	
	
    	Sound (	"..\\..\\Acela\\Sound\\AcelaEng.sms" )
      )
Engine ( SS9G0094k541
    Wagon ( SS9G0094k541 )
    Type ( Electric )
    MaxPower ( 5400kW )
    MaxForce ( 486kN#est )
    MaxContinuousForce ( 369kN )
    MaxVelocity ( 180m/s )
    MaxCurrent ( 870A )
    WheelRadius ( 0.55m )
    Sanding ( 1e9mph )
    NumWheels ( 1 )

    CabView ( SS9G.cvf )

    AirBrakesAirCompressorPowerRating( 3.5 )
    AirBrakesMainMinResAirPressure( 0 )
    AirBrakesMainMaxAirPressure( 140 )
    AirBrakesMainResVolume( 10 )
    AirBrakesAirCompressorWattage( 19000 )
    AirBrakesCompressorRestartPressure( 130 )
    AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.5 )
    AirBrakesHasLowPressureTest( 1 )
    AirBrakesIsCompressorElectricOrMechanical( 1 )

    EngineBrakesControllerHasProportionalBrake( 1 )
    EngineBrakesProportionalBrakeLag( 1 )

    TrainBrakesControllerMinPressureReduction( 6 )
    TrainBrakesControllerMaxApplicationRate( 10 )
    TrainBrakesControllerMaxReleaseRate( 2 )
    TrainBrakesControllerEmergencyApplicationRate( 40 )
    TrainBrakesControllerMinSystemPressure( 0 )
    TrainBrakesControllerMaxSystemPressure( 110 )
    TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
    TrainBrakesControllerFullServicePressureDrop( 26 )

    DynamicBrakesMinUsableSpeed( 5 )
    DynamicBrakesMaximumEffectiveSpeed( 25 )
    DynamicBrakesMaximumForce( 20000 )
    DynamicBrakesResistorCurrentLimit ( 5000 )
    DynamicBrakesCutInSpeed( 8 )
    DynamicBrakesMaxAirBrakePressure ( 15 )
    DynamicBrakesFadingSpeed( 25 )
    DynamicBrakesDelayTimeBeforeEngaging ( 10 )
    DynamicBrakesMaximumSpeedForFadeOut ( 65 )
    DynamicBrakesEffectAtMaximumFadeOut( 0 )
    DynamicBrakesHigherSpeedCurveExponent( 1 )
    DynamicBrakesLowerSpeedCurveExponent( 1 )
    DynamicBrakesNumberOfControllerNotches( 8 )

    BrakesEngineBrakeType( "Air_twin_pipe"  )
    BrakesTrainBrakeType( "Air_twin_pipe" )
    BrakesEngineControllers( "Train, Dynamic, Blended" )
    
    DoesBrakeCutPower( 1 )
    DoesHornTriggerBell( 0 )
    BrakeCutsPowerAtBrakeCylinderPressure( 15 )
    
	EmergencyStopMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 45 )
		MonitoringDeviceAlarmTimeLimit( 37 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 220 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 1 ) 
		MonitoringDeviceResetOnResetButton( 0 )
		)


    Sound ( "..\\..\\Acela\\Sound\\AcelaCab.sms" )
    Name ( "SS9G 0094 k541" )
    Description (
	"The Amtrak® Acela(SM) Express, a new high-speed electric trainset. Each Acela Express trainset "+
	"consists of five passenger cars, a cafe car, and two 6,000 hp Power Cars (locomotives), one at "+
	"each end.\n\n"+
	"Locomotive type: Bombardier ALSTOM Consortium high-speed electric power car\n\n"+
	"Power source: Catenary from stationary electric generator\n\n"+
	"Power, each power car: 6,169 hp; 4,600 kilowatts\n\n"+
	"Max. speed: 165 mph (265.4 km/h)\n\n"+
	"Height: 14 ft. 2 in. (4.3 m)\n\n"+
	"Width: 10 ft. 5 in. (3.2 m)\n\n"+
	"Length, each power car: 69 ft. 7 in. (21.2 m)\n\n"+
	"Length, trainset: 663 ft. 9 in. (202.3 m)\n\n"+
	"Weight, each power car: 200,000 lb (90,720 kg)\n\n"+
	"Weight, trainset: 1,171,000 lb (531,156.7 kg)\n\n"+
	"Max. short time tractive effort, each power car: 49,000 lb (22,226 kg) (Front & rear power car "+
	"combined effort: 98,000 lb)\n\n"+
	"Wheel configuration, each power car: Eight 40-inch diameter wheels in B-B configuration (two "+
	"sets of two driven axles)"
    )
    EngineOperatingProcedures (
    "To move forward\n"+
    "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
    "2.	Press the W key to move the Reverser to Forward.\n"+
    "3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
    "4.	Press the D key to move increase the throttle setting.\n\n"+  
    "To slow the train\n"+
    "1.	Press the A key to move the throttle to a lower setting.\n"+
    "2.	Use the brakes to further reduce speed if desired.\n\n"+   
    "To apply the train brakes\n"+
    "1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
    "To release the train brakes\n"+
    "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
    "To activate emergency braking\n"+
    "1.	Press the A key to reduce the throttle to Idle.\n"+
    "2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
    "To back up\n"+
    "1.	Bring your train to a full stop.\n"+
    "2.	Press the S key to move the Reverser to the Reverse position.\n"+
    "3.	Press the ; (SEMICOLON)  to release the brakes.\n"+
    "4.	Slowly advance the throttle lever (D key).\n\n"+
    "To load and unload passengers\n"+
    "1. Stop at a station.\n"+
    "2. Press the ENTER key.\n"+
    "3. Wait for the 'permission to depart' signal.\n"+
    "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading."
    ) 
    
    EngineControllers (
        Throttle ( 0 1 0.025 0
            NumNotches ( 0 )
        )
        Brake_Train ( 0 1 0.0125 0.5 
            NumNotches ( 6
                Notch ( 0       0 TrainBrakesControllerReleaseStart )
                Notch ( 0.2	0 TrainBrakesControllerHoldLappedStart )
                Notch ( 0.25    1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                Notch ( 0.85    0 TrainBrakesControllerSuppressionStart )
                Notch ( 0.9     0 TrainBrakesControllerContinuousServiceStart )
                Notch ( 0.95    0 TrainBrakesControllerEmergencyStart )
            )
        )
        Brake_Dynamic ( 0 1 0.0125 0 
            NumNotches( 0 )
        )
        DirControl ( -1 0 1 1 )
        EmergencyStopResetToggle( 0 1 0 )
        EmergencyStopToggle( 0 1 0 )
        AWS ( 0 1 0 )
        Sanding ( 0 1 0 )
        Horn ( 0 1 0 )
        Vigilance ( 0 1 0 )
        PantographToggle1 ( 0 1 1 )
        Headlights ( 0 0.25 1 0 )
        Wipers ( 0 1 0 )
        BellToggle( 0 1 0 )
    )
)


