SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( DF11G_0147
	Type ( Engine )
	WagonShape ( DF11G_0147.s )
	Size ( 3.13m 4.755m 22.3m )
	comment( Made by JINJIN )
	Mass ( 138.0t )
	WheelRadius ( 0.575m )
	InertiaTensor ( Box (3.1m 4.6m 22.3m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 9.8e5N/m 1.76e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 2.45e7N 1.78e6N )
			r0 ( 0cm 4cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 9.8e5N/m 1.76e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 2.45e6N 1.78e6N )
			r0 ( 0cm 4cm )
		)
		Comment ( CouplingHasRigidConnection ( 1 ) )
		Velocity ( -0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 9.8e5N/m 9.8e5N/m )
			Damping ( 1.7e6N/m/s 1.7e6N/m/s )
			r0 ( 20cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	
	Adheasion ( 5000 10000 20000 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 230kn)
	DerailBufferForce ( 156kN )
	NumWheels ( 12 )
	Friction (
	11N/m/s		1		 60mph	11N/m/s                        1
		2.1N/rad/s		1		1rad/s		0		1
	)
	AntiSlip (  )

	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )

	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce ( 400kN )
	
	EmergencyBrakeResMaxPressure( 210 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 30 )
	MaxApplicationRate( 25 )
	MaxAuxilaryChargingRate( 20 )
	EmergencyResCapacity( 10 )
	EmergencyResChargingRate( 25 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	IntakePoint ( -3.33 0.4 FuelDiesel )
	IntakePoint ( 3.33 0.4 FuelDiesel )

	Lights	(	7
		Light	(
			comment( Sphere of light )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffff )
					Position ( 0.0 3.5 20 )
					Transition ( 0 )
					Radius ( 400.0 )
					Angle ( 15.0 )
					)
				)
			)
		Light	(
			comment( Head light left dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2)
				Unit ( 2 )
				)
			FadeIn	( 3 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b )
					Position ( 0.86 2 11 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0 0 0))
				)
			)
		Light	(
			comment( Head light right dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 3 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b)
					Position ( -0.86 2 11 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0 0 0 ))
				)
			)
		Light	(
			comment( Head light right bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 2.5 )
			FadeOut	( 1.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffcc)
					Position ( 0.86 2 11 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( 0 0 0 ))
				)
			)
		Light	(
			comment( Head light left bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 2.5 )
			FadeOut	( 1.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffcc )
					Position ( -0.86 2 11 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( 0 0 0 )
					)
				)
			)		
		Light	(
			comment( top light bright)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 5.5 )
			FadeOut	( 5.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffcc )
					Position ( 0 4.15 9.6 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( .8 )
					Elevation ( -50 -50 -50)
					)
				)
			)
	Light	(
			comment( back light)
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Unit ( 2 )
				)
			FadeIn	( 3.5 )
			FadeOut	( 3.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 00000000 )
					Position ( -0.831 2.079 -11 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( .3 )
					Elevation ( 0 0 0 )
					)
				)
			)

	
		)

    	Sound (	"DF11Geng.sms" )
	)

Engine ( DF11G_0147
	Effects
		(
		DieselSpecialEffects
			(
				comment
				(
					the format of these little blocks is as follow:

					offset.x offset.y offset.z
					normal.x normal.y normal.z
					width in metres

					defining the offset from the shape pivot point
					where steam / smoke should appear, the direction
					it should go and the width of the nozzle
				)

				Exhaust1
				(
					0.0  4.8 1.7
					0 1 0
					0.2
				)
				Exhaust2
				(
					0.0 4.8 -1.5
					0 1 0
					0.2
				)
			)
        	)
        
	Wagon ( DF11G_0147 )
	Type ( Diesel )
	MaxPower ( 3610kw )
	comment( est estimated by comparision with dash9 )
	MaxForce ( 195kN )	
	MaxContinuousForce ( 125kN )
	MaxVelocity ( 170kmh )
	MaxCurrent ( 3000A ) 
	WheelRadius ( 0.575m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 1e9mph )
	NumWheels ( 1 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )
 	CabView ( DF11GA.cvf )
        HeadOut ( -1.8 3.1 9.3 )
	MaxDieselLevel ( 3600gal )
	DieselUsedPerHourAtMaxPower ( 60gal )
	DieselUsedPerHourAtIdle ( 10gal )

	AirBrakesAirCompressorPowerRating( 1.2 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 200 )
	AirBrakesMainResVolume( 8 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 87 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.22 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMinPressureReduction( 6 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 20 )
	TrainBrakesControllerMaxApplicationRate( 2 )
	EngineBrakesControllerMaxReleaseRate( 15 )
	TrainBrakesControllerMaxReleaseRate( 4 )
	EngineBrakesControllerEmergencyApplicationRate( 50 )
	TrainBrakesControllerEmergencyApplicationRate( 50 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	TrainBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	EngineBrakesControllerFullServicePressureDrop( 26 )
	TrainBrakesControllerFullServicePressureDrop( 26 )


	DynamicBrakesMinUsableSpeed( 5 )
	DynamicBrakesMaximumEffectiveSpeed( 190 )
	DynamicBrakesMaximumForce( 55000 )
	DynamicBrakesResistorCurrentLimit ( 5000 )
	DynamicBrakesCutInSpeed( 8 )
	DynamicBrakesMaxAirBrakePressure ( 15 )
	DynamicBrakesFadingSpeed( 25 )
	DynamicBrakesDelayTimeBeforeEngaging ( 8 )
	DynamicBrakesMaximumSpeedForFadeOut ( 65 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 10 )


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
        BrakesEngineControllers( "Independent, Train, Dynamic" )
        
        EngineBrakesControllerDirectControlExponent( 1 )

	MaxDieselLevel ( 2000gal )
	DieselUsedPerHourAtMaxPower ( 60gal )
	DieselUsedPerHourAtIdle ( 10gal )

	DieselSmokeEffectInitialMagnitude( 1.5 )
	DieselSmokeEffectMaxMagnitude( 1.5 )
	DieselSmokeEffectInitialSmokeRate( 0.5 )
	DieselSmokeEffectMaxSmokeRate( 2.5 )	
	
	DieselEngineIdleRPM( 255 )
	DieselEngineMaxRPM( 904 )
	DieselEngineSpeedOfMaxTractiveEffort( 20.8kph )        
        DieselEngineMaxRPMChangeRate( 40 )

	DoesHornTriggerBell( 0 )

	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 0 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)

	AWSMonitor(
		MonitoringDeviceMonitorTimeLimit( -1 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)
	
	EngineVariables( 3600 )
			
        EngineControllers (
           Throttle ( 0 1 0.0125 0 
                NumNotches ( 17 
                    Notch ( 0        0 Dummy )
                    Notch ( 0.01     0 Dummy )
                    Notch ( 0.07     0 Dummy )
                    Notch ( 0.13     0 Dummy )
                    Notch ( 0.18     0 Dummy )
                    Notch ( 0.25     0 Dummy )
                    Notch ( 0.31     0 Dummy )
                    Notch ( 0.36     0 Dummy )
                    Notch ( 0.42     0 Dummy )
                    Notch ( 0.48     0 Dummy )
                    Notch ( 0.54     0 Dummy )
                    Notch ( 0.61     0 Dummy )
                    Notch ( 0.69     0 Dummy )
                    Notch ( 0.76     0 Dummy )
                    Notch ( 0.82     0 Dummy )
                    Notch ( 0.88     0 Dummy )
                    Notch ( 1        0 Dummy)
                    )
            )
            Brake_Engine ( 0 1 0.075 0 
                NumNotches ( 1
                    Notch( 0  1 Dummy )
                )
            )
            Brake_Train ( 0 1 0.025 0.5 
                NumNotches ( 6
                    Notch( 0.0  0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch( 0.2  0 TrainBrakesControllerReleaseStart )
                    Notch( 0.3  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch (0.8 0 TrainBrakesControllerFullServiceStart )
                    Notch( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch( 1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Dynamic ( 0 1 0.11 0 
                NumNotches ( 10 
                	Notch ( 0       0 Dummy )
                    	Notch ( 0.11    0 Dummy )
                  	Notch ( 0.22    0 Dummy )
                   	Notch ( 0.33    0 Dummy )
                   	Notch ( 0.44    0 Dummy )
                   	Notch ( 0.55    0 Dummy )
                   	Notch ( 0.66    0 Dummy )
                   	Notch ( 0.77    0 Dummy )
                   	Notch ( 0.88    0 Dummy )
                   	Notch ( 1       0 Dummy )
                )
            )

            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
        
    	Sound (	"DF11GCab.sms" )
    	Name ("DF11G_0147")
    	Description (
	" \n\n"+
	" \n\n"+
	" \n\n"+
	" \n\n"+
	" \n\n"
	""
    	)
    	EngineOperatingProcedures (
    	"To move forward\n"+
	"1.	Press the W key to move the Reverser to Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"4.	Press the D key to move the throttle from Idle to Notch 1.\n"+
	"5.	Gradually increase power (D key), one notch at a time, until your train reaches the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the dynamic brakes\n"+
	"1.	Press the A key to move the throttle to the Idle position.\n"+
	"2.	Wait for 10 seconds, then press the . (PERIOD) key to advance the Dynamic Brake handle from Off to the Setup position. After allowing a few seconds for braking circuit setup, press the . (PERIOD) key again to set the desired level of dynamic braking (Levels 1 - 8).\n\n"+
	"To release the dynamic brakes\n"+
	"1. Press the D key to move the throttle towards Idle.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
	"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
    	) 
)

