SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( DFH21_051
	Type ( Engine )
	WagonShape ( DFH21_051.s )
	Size ( 3.046m 3.793m 12.6m)
	Mass ( 69t )
	WheelRadius ( 0.5025m )
	InertiaTensor ( Box (3.046m 3.793m 12.6m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 9.8e5N/m 1.76e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 2.45e7N 1.78e6N )
			r0 ( 0cm 4cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 9.8e5N/m 1.76e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 2.45e6N 1.78e6N )
			r0 ( 0cm 4cm )
		)
		Comment ( CouplingHasRigidConnection ( 1 ) )
		Velocity ( -0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 9.8e5N/m 9.8e5N/m )
			Damping ( 1.7e6N/m/s 1.7e6N/m/s )
			r0 ( 20cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*250e3lbs )
	DerailBufferForce ( 280kN )
	NumWheels (	12 )
	Friction (
		155N/m/s		1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)
	AntiSlip ( 1 )

	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )

	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce ( 200kN )
	
	EmergencyBrakeResMaxPressure( 110 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 30 )
	MaxApplicationRate( 25 )
	MaxAuxilaryChargingRate( 20 )
	EmergencyResCapacity( 10 )
	EmergencyResChargingRate( 25 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	IntakePoint ( -3.33 0.4 FuelDiesel )
	IntakePoint ( 3.33 0.4 FuelDiesel )

	Lights	(	8
		Light	(
			comment( Sphere of light )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffff )
					Position ( 0.0 3.5 20 )
					Transition ( 0 )
					Radius ( 200.0 )
					Angle ( 15.0 )
					)
				)
			)
		Light	(
			comment( Head light top dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80f5c37b )
					Position ( 0.00 3.5 5.9 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
		Light	(
			comment( Head light top bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b)
					Position ( 0.00 3.5 5.89 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)
		Light	(
			comment( Head light right bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b )
					Position ( 1.20 1.51 5.82 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( Head light left bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fff5c37b )
					Position ( -1.20 1.51 5.82 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)		
		Light	(
			comment( Rear red left light )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.71 1.59 -5.32 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3)
					)
				)
			)

		Light	(
			comment( Rear right red light )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.71 1.59 -5.32 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		)
    	Sound (	"DFH21eng.sms" )

	)

Engine ( DFH21_051
	Effects
		(
		DieselSpecialEffects
			(
				Exhaust1
				(
					-0.0  3.873 1.4
					0 1 0
					0.1
				)

			)
        	)
        
	Wagon ( DFH21_051 )
	Type ( Diesel )
	MaxPower ( 640kw )
	MaxForce ( 194kN )	
	MaxContinuousForce ( 149kN )
	MaxVelocity ( 50kmh )
	MaxCurrent ( 1680A ) 
	WheelRadius ( 0.5025m )
	Sanding ( 1e9mph )
	NumWheels ( 1 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )

 	CabView ( DFH21.cvf )
	HeadOut ( 1.8 3.0 4.4 )
	MaxDieselLevel ( 3600gal )
	DieselUsedPerHourAtMaxPower ( 60gal )
	DieselUsedPerHourAtIdle ( 10gal )

	AirBrakesAirCompressorPowerRating( 1.2 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 90 )
	AirBrakesMainResVolume( 8 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 87 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.22 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMinPressureReduction( 6 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 20 )
	TrainBrakesControllerMaxApplicationRate( 20 )
	EngineBrakesControllerMaxReleaseRate( 15 )
	TrainBrakesControllerMaxReleaseRate( 4 )
	EngineBrakesControllerEmergencyApplicationRate( 50 )
	TrainBrakesControllerEmergencyApplicationRate( 50 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	TrainBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	EngineBrakesControllerFullServicePressureDrop( 26 )
	TrainBrakesControllerFullServicePressureDrop( 26 )


	DynamicBrakesMinUsableSpeed( 5 )
	DynamicBrakesMaximumEffectiveSpeed( 80 )
	DynamicBrakesMaximumForce( 55000 )
	DynamicBrakesResistorCurrentLimit ( 5000 )
	DynamicBrakesCutInSpeed( 8 )
	DynamicBrakesMaxAirBrakePressure ( 15 )
	DynamicBrakesFadingSpeed( 25 )
	DynamicBrakesDelayTimeBeforeEngaging ( 8 )
	DynamicBrakesMaximumSpeedForFadeOut ( 65 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 10 )


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
        BrakesEngineControllers( "Independent, Train, Dynamic" )
        
        EngineBrakesControllerDirectControlExponent( 1 )

	MaxDieselLevel ( 2000gal )
	DieselUsedPerHourAtMaxPower ( 60gal )
	DieselUsedPerHourAtIdle ( 10gal )

	DieselSmokeEffectInitialMagnitude( 1.0)
	DieselSmokeEffectMaxMagnitude( 1.0 )
	DieselSmokeEffectInitialSmokeRate( 0.2 )
	DieselSmokeEffectMaxSmokeRate( 1.0 )	
	
	DieselEngineIdleRPM( 255 )
	DieselEngineMaxRPM( 1000 )
	DieselEngineSpeedOfMaxTractiveEffort( 20.8kph )        
        DieselEngineMaxRPMChangeRate( 40 )

	DoesHornTriggerBell( 0 )

	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 0 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)

	AWSMonitor(
		MonitoringDeviceMonitorTimeLimit( -1 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)
	
      EngineControllers (
            Throttle ( 0 1 0.04 0 
                NumNotches ( 0 )
            )
            Brake_Engine ( 0 1 0.2 0 
                NumNotches ( 1
                    Notch( 0  1 Dummy )
                )
            )
            Brake_Engine ( 0 1 0.0125 0 
                NumNotches ( 1
                    Notch( 0  1 Dummy )
                )
            )
            Brake_Train ( 0 1 0.0125 0.75 
                NumNotches ( 5
                    Notch( 0    0 TrainBrakesControllerReleaseStart )
                    Notch( 0.3  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch( 0.85 0 TrainBrakesControllerSuppressionStart )
                    Notch( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch( 0.95 0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Dynamic ( 0 1 0.11 0 
                NumNotches ( 10 
                	Notch ( 0       0 Dummy )
                    	Notch ( 0.11    0 Dummy )
                  	Notch ( 0.22    0 Dummy )
                   	Notch ( 0.33    0 Dummy )
                   	Notch ( 0.44    0 Dummy )
                   	Notch ( 0.55    0 Dummy )
                   	Notch ( 0.66    0 Dummy )
                   	Notch ( 0.77    0 Dummy )
                   	Notch ( 0.88    0 Dummy )
                   	Notch ( 1       0 Dummy )
                )
            )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
        
    	Sound (	"DFH21cab.sms" )
    	Name ( "DFH21_051" )
    	Description (
	" \n昆明铁路局DFH21米轨内燃机车\n"+
	" \nDF4D3295制作\n"+
        " \n本插件属于免费插件，严禁用于商业用途\n"+
	" \n东方红21型是高原米轨通用型内燃机车，由四方机车车辆工厂于1976年设计，1977年试制投产，1982年又进行改进。机车标称功率是640kW，最大速度50km/h，车长12000mm，轴式B-B。
\n"+
	" \n首台制成年份：1977年
　　柴油机装车功率：1100马力
　　传动方式：液力
　　用途：客货运、调车
　　轴式：B-B
　　轨距：1000毫米
　　整备重量：69吨
　　轴重：15吨
　　构造速度：50公里/小时
　　持续速度：小于12公里/小时
　　起动牵引力：19800公斤
　　持续牵引力：14000公斤
　　轮径：915毫米
　　机车轴距：8200毫米
　　转向架轴距：2200毫米
　　转向架中心线间距：6000毫米
　　车钩中心线间距：12676毫米
　　通过最小曲线半径：70米
　　最大高度：3793毫米
　　最大宽度：3046毫米
　　燃油储备量：2吨
　　水/砂储备量：0.5/1吨 
　　柴油机型号：12V180ZJA
　　液力装置型号：SF2010Z-2 \n"
	""
    	)
    	EngineOperatingProcedures (
    	" "
    	) 

)

